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[bookmark: _GoBack]VARIANT 03 - Square Flange Female Receptacle, for PCB TRANSMISSION Line WITH Ø PIN 1.73mm
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NOTES:
0. Accept pin Ø 1.73mm.
		Symbols
	Dimensions (mm)
	Remarks

	
	Min
	Max
	

	A
	19.9
	20.3
	

	B
	13.6
	13.8
	

	C
	4.4
	4.6
	

	D
	21.9
	22.2
	

	E
	4.15
	4.35
	

	F
	13.45
	13.55
	

	G
	18.9
	19.1
	

	ØH
	3.1
	3.3
	4 Holes	

	ØJ
	24.3
	24.6
	


	


	Electrical Characteristics
	Values
	Units

	Voltage Standing Wave Ratio (VSWR)
	≤ 1.1 + 0.02 x f (GHz)
	-

	RF Insertion loss
	≤ 0.04 x f (GHz)
	dB

	RF Leakage
	≤ -115 + f (GHz)
	dBi

	Voltage Proof
	≥ 1500
	Vrms

	Corona
	≥ Pco at 1GHz (see Table 1(b))
	W

	Multipaction Threshold (pulse width 20µs; PRF: 1kHz)
	≥ 2000 at 1GHz
	Wpp

	
	
	

	Mechanical Characteristics
	Values
	Units

	Centre Contact Retention Force (Axial)
	≥ 27.2
	N

	Centre Contact Retention Torque (Rotational)
	≥ 2.8
	N.cm

	Cable Retention Force (Axial)
	Not applicable
	N

	Cable Retention Torque (Rotational)
	Not applicable
	N.cm

	Weight
	≤ 16
	g

	
	
	

	Other Characteristics
	Values
	Units

	Operating Temperature Range
	-65 to +165
	°C

	Leakage Rate (Panel-sealed Connectors)
	Not applicable
	-

	Leakage Rate (Hermetic Sealed Connector)
	Not applicable
	-

	Solderability
	Not Applicable
	-

	Soldering Proof
	Not Applicable
	-

	Cables used
	Not applicable
	-
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Ref. Plane.
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